$$ 06-20-00 vens created; test files

Curve fit in GPost test:

Curve fit done in GPost and MCD format done in GPost:

APT files:

1. t1.apt,p01,f01 - arcfit apt file f01=dummy
   $$CRVFIT/ARC,ON
   INTCOM(4334)=1
   DBLCOM(0994)=1

2. t2.apt,p02,f02 - arcfit with helix apt file f02=dummy
   $$CRVFIT/ARC,ON
   INTCOM(4334)=1
   DBLCOM(0994)=1
   $$CRVFIT/ARCSLP,ON
   DBLCOM(0995)=1

3. t3.apt,p03,f03 - spline fit apt file f03=fanuc
   $$CRVFIT/SPLINE,ON
   INTCOM(4334)=1
   DBLCOM(0996)=1

4. t4.apt,p04,f04 - spline fit with cutcom apt file f04=fanuc
   $$CRVFIT/SPLINE,ON
   INTCOM(4334)=1
   DBLCOM(0996)=1

5. t5.apt,p05,f05 - spline and arcfit butterfly apt file f05=fanuc
   $$CRVFIT/ARC,ON
   INTCOM(4334)=1
   DBLCOM(0994)=1
   $$CRVFIT/SPLINE,ON
   DBLCOM(0996)=1

6. t6.apt,p06,f06 - spline fit of bsurf apt file f06=fanuc
   $$CRVFIT/SPLINE,ON
   INTCOM(4334)=1
   DBLCOM(0996)=1

7. t7.apt,p07,f07 - arc fit of bsurf apt file f07=dummy
   $$CRVFIT/ARC,ON
   INTCOM(4334)=1
   DBLCOM(0994)=1

8. t8.apt,p08,f08 - spline fit of bsurf apt file f06=siemens poly
   $$CRVFIT/SPLINE,ON
   INTCOM(4334)=1
   DBLCOM(0996)=1
   $$CRVFIT/TYPE,1
   DBLCOM(0997)=1

CAD files:

1. f11.apt,p11,f11 - spline fit of cad file f11=fanuc nurb
   $$CRVFIT/SPLINE,ON
   INTCOM(4334)=1
   DBLCOM(0996)=1

2. s12.apt,p12,f12 - spline fit of cad file f12=siemens nurb
   $$CRVFIT/SPLINE,ON
   INTCOM(4334)=1
   INTCOM(4335)=1
   DBLCOM(0996)=1

3. h13.apt,p13,f13 - spline fit of cad file f13=heidenhein nurb
   $$CRVFIT/SPLINE,ON
   INTCOM(4334)=1
   INTCOM(4335)=2
   DBLCOM(0996)=1

4. s14.apt,p14,f14 - spline fit of cad file f14=siemens poly
   $$CRVFIT/SPLINE,ON
   INTCOM(4334)=1
   DBLCOM(0996)=1
   $$CRVFIT/TYPE,1
   DBLCOM(0997)=1

5. s15.apt,p15,f15 - arc fit of cad file f15=siemens CIP arc
   $$CRVFIT/ARC,ON
   INTCOM(4334)=1
   DBLCOM(0994)=1
   $$CRVFIT/XYZ,2
   DBLCOM(0997)=2

6. f16.apt,f16,f16 - arc fit of cad file f16=fanuc g3.4 arc
   $$CRVFIT/ARC,ON
   INTCOM(4334)=1
   DBLCOM(0994)=1
   $$CRVFIT/XYZ,1
   DBLCOM(0997)=1

end
